## How do I Use the serial port to control a fan

For our Q3UPT machine equipped with cooling fan, the serial port can be used to control the start and stop of the fan. The following is the procedure you need to perform.

1. Open the serial port device with sdk aar.

2. Send control commands.

3. Check the command response.

4. Close the serial port device.

We provide a code snippet and a simple demo apk that you can refer.